Note: Version 1.1.2 drastically improves keyboard and screen reader accessibility for the `md-chips` component. In order to achieve this, the behavior has changed to also select and highlight the newly appended chip for `300ms` before re-focusing the text input.

Please see the documentation for more information and for the new `md-chip-append-delay` option which allows you to customize this delay.