/** @page primerjtag OpenOCD JTAG Primer

JTAG is unnecessarily confusing, because JTAG is often confused with
boundary scan, which is just one of its possible functions.

JTAG is simply a communication interface designed to allow communication
to functions contained on devices, for the designed purposes of
initialisation, programming, testing, debugging, and anything else you
want to use it for (as a chip designer).

Think of JTAG as I2C for testing.  It doesn't define what it can do,
just a logical interface that allows a uniform channel for communication.

See @par
	http://en.wikipedia.org/wiki/Joint_Test_Action_Group

@image html jtag-state-machine-large.png

The first page (among other things) shows a logical representation
describing how multiple devices are wired up using JTAG.  JTAG does not
specify, data rates or interface levels (3.3V/1.8V, etc) each device can
support different data rates/interface logic levels.  How to wire them
in a compatible way is an exercise for an engineer.

Basically TMS controls which shift register is placed on the device,
between TDI and TDO.  The second diagram shows the state transitions on
TMS which will select different shift registers.

The first thing you need to do is reset the state machine, because when
you connect to a chip you do not know what state the controller is in,you need
to clock TMS as 1, at least 5 times.  This will put you into "Test Logic
Reset" State.  Knowing this, you can, once reset, then track what each
transition on TMS will do, and hence know what state the JTAG state
machine is in.

There are 2 "types" of shift registers.  The Instruction shift register
and the data shift register.  The sizes of these are undefined, and can
change from chip to chip.  The Instruction register is used to select
which Data register/data register function is used, and the data
register is used to read data from that function or write data to it.

Each of the states control what happens to either the data register or
instruction register.

For example, one of the data registers will be known as "bypass" this is
(usually) a single bit which has no function and is used to bypass the
chip.  Assume we have 3 identical chips, wired up like the picture(wikipedia)
and each has a 3 bits instruction register, and there are 2 known
instructions (110 = bypass, 010 = "some other function") if we want to use
"some other function", on the second chip in the line, and not change
the other chips we would do the following transitions.

From Test Logic Reset, TMS goes:

  0 1 1 0 0

which puts every chip in the chain into the "Shift IR state"
Then (while holding TMS as 0) TDI goes:

  0 1 1  0 1 0  0 1 1

which puts the following values in the instruction shift register for
each chip [110] [010] [110]

The order is reversed, because we shift out the least significant bit
first.  Then we transition TMS:

  1 1 1 0 0

which puts us in the "Shift DR state".

Now when we clock data onto TDI (again while holding TMS to 0) , the
data shifts through the data registers, and because of the instruction
registers we selected ("some other function" has 8 bits in its data
register), our total data register in the chain looks like this:

  0 00000000 0

The first and last bit are in the "bypassed" chips, so values read from
them are irrelevant and data written to them is ignored.  But we need to
write bits for those registers, because they are in the chain.

If we wanted to write 0xF5 to the data register we would clock out of
TDI (holding TMS to 0):

  0 1 0 1 0 1 1 1 1 0

Again, we are clocking the least-significant bit first.  Then we would
clock TMS:

  1 1 0

which updates the selected data register with the value 0xF5 and returns
us to run test idle.

If we needed to read the data register before over-writing it with F5,
no sweat, that's already done, because the TDI/TDO are set up as a
circular shift register, so if you write enough bits to fill the shift
register, you will receive the "captured" contents of the data registers
simultaneously on TDO.

That's JTAG in a nutshell.  On top of this, you need to get specs for
target chips and work out what the various instruction registers/data
registers do, so you can actually do something useful.  That's where it
gets interesting.  But in and of itself, JTAG is actually very simple.

@section primerjtag More Reading

A separate primer contains information about @subpage primerjtagbs for
developers that want to extend OpenOCD for such purposes.

 */
/** @page primerjtagbs JTAG Boundary Scan Primer

The following page provides an introduction on JTAG that focuses on its
boundary scan capabilities: @par
http://www.engr.udayton.edu/faculty/jloomis/ece446/notes/jtag/jtag1.html

OpenOCD does not presently have clear means of using JTAG for boundary
scan testing purposes; however, some developers have explored the
possibilities.  The page contains information that may be useful to
those wishing to implement boundary scan capabilities in OpenOCD.

@section primerbsdl The BSDL Language

For more information on the Boundary Scan Description Language (BSDL),
the following page provides a good introduction: @par
http://www.radio-electronics.com/info/t_and_m/boundaryscan/bsdl.php

@section primerbsdlvendors Vendor BSDL Files

NXP LPC: @par
http://www.standardics.nxp.com/support/models/lpc2000/

Freescale PowerPC: @par
http://www.freescale.com/webapp/sps/site/overview.jsp?code=DRPPCBSDLFLS

Freescale i.MX1 (too old): @par
http://www.freescale.com/webapp/sps/site/prod_summary.jsp?code=i.MX1&nodeId=0162468rH311432973ZrDR&fpsp=1&tab=Design_Tools_Tab

Renesas R32C/117: @par
http://sg.renesas.com/fmwk.jsp?cnt=r32c116_7_8_root.jsp&fp=/products/mpumcu/m16c_family/r32c100_series/r32c116_7_8_group/
- The device page does not come with BSDL file; you have to register to
  download them. @par
  http://www.corelis.com/support/BSDL.htm

TI links theirs right off the generic page for each chip;
this may be the case for other vendors as well.  For example:

- DaVinci DM355 -- http://www.ti.com/litv/zip/sprm262b
- DaVinci DM6446
  - 2.1 silicon -- http://www.ti.com/litv/zip/sprm325a
  - older silicon -- http://www.ti.com/litv/zip/sprm203
- OMAP 3530
  - CBB package -- http://www.ti.com/litv/zip/sprm315b
    - 515 ball s-PGBA, POP, 0.4mm pitch
  - CUS package -- http://www.ti.com/litv/zip/sprm314a
    - 515 ball s-PGBA, POP, 0.5mm pitch
  - CBC package -- http://www.ti.com/litv/zip/sprm346
    - 423 ball s-PGBA, 0.65mm pitch

Many other files are available in the "Semiconductor Manufacturer's BSDL
files" section of the following site: @par
http://www.freelabs.com/~whitis/electronics/jtag/

 */
/** @file
This file contains the @ref primerjtag and @ref primerjtagbs page.
 */
