# Test cases

## Test case results

The test results are stored in seperate documents. One document for each subversion number.

Test results | comment
SAM7 R607 | PASS
STR710 R607 | PASS
template | Test results template

## Vocabulary

Passed version | The latest branch and version on which the test is known to pass
Broken version | The latest branch and version on which the test is known to fail. n/a when older than passed version.
ID | A unqiue ID to refer to a test. The unique numbers are maintained in this file. Note that the same test can be run on different hardware/interface. Each combination yields a unique id.
Test case | An atomic entity that describes the operations needed to test a feature or only a part of it. The test case should: be uniquely identifiable define the complete prerequisites of the test (eg: the target, the interface, the initial state of the system) define the input to be applied to the system in order to execute the test define the expected output contain the output resulted by running the test case contain the result of the test (pass/fail)
Test suite | A (completable) collection of test cases
Testing | Testing refers to running the test suite for a specific revision of the software, for one or many targets, using one or many JTAG interfaces. Testing should be be stored along with all the other records for that specific revision. For releases, the results can be stored along with the binaries
Target = ANY | Any target can be used for this test
Interface = ANY | Any interface can be used for this test
Target = "reset_config srst_and_trst" | Any target which supports the reset_config above

# Test cases

## Connectivity

ID | Target | Interface | Description | Initial state | Input | Expected output | Pass/Fail
CON001 | ALL | ALL | Telnet connection | Power on, jtag target attached | On console, type `telnet ip port` | `Open On-Chip Debugger >` | PASS/FAIL
CON002 | ALL | ALL | GDB server connection | Power on, jtag target attached | On GDB console, type `target remote ip:port` | `Remote debugging using 10.0.0.73:3333` | PASS/FAIL

## Reset

ID | Target | Interface | Description | Initial state | Input | Expected output | Pass/Fail
RES001 | Fill in! | Fill in! | Reset halt on a blank target | Erase all the content of the flash | Connect via the telnet interface and type `reset halt` | Reset should return without error and the output should contain `target state: halted pc = 0` | PASS/FAIL
RES002 | Fill in! | Fill in! | Reset init on a blank target | Erase all the content of the flash | Connect via the telnet interface and type `reset init` | Reset should return without error and the output should contain `executing reset script 'name_of_the_script'` | PASS/FAIL
RES003 | Fill in! | Fill in! | Reset after a power cycle of the target | Reset the target then power cycle the target | Connect via the telnet interface and type `reset halt` after the power was detected | Reset should return without error and the output should contain `target state: halted` | PASS/FAIL
RES004 | ARM7/9,reset_config srst_and_trst | ANY | Reset halt on a blank target where reset halt is supported | Erase all the content of the flash | Connect via the telnet interface and type `reset halt` | Reset should return without error and the output should contain `target state: halted pc = 0` | PASS/FAIL
RES005 | arm926ejs,reset_config srst_and_trst | ANY | Reset halt on a blank target where reset halt is supported. This target has problems with the reset vector catch being disabled by TRST | Erase all the content of the flash | Connect via the telnet interface and type `reset halt` | Reset should return without error and the output should contain `target state: halted pc = 0` | PASS/FAIL

## JTAG Speed

ID | Target | Interface | Description | Initial state | Input | Expected output | Pass/Fail
RES001 | Fill in! | Fill in! | 16MHz on normal operation | Reset init the target according to RES002 | Exercise a memory access over the JTAG, for example `mdw 0x0 32` | The command should run without any errors. If any JTAG checking errors happen, the test failed | PASS/FAIL

## Debugging

ID | Target | Interface | Description | Initial state | Input | Expected output | Pass/Fail
DBG001 | Fill in! | Fill in! | Load is working | Reset init is working, RAM is accesible, GDB server is started | On the console of the OS: `arm-elf-gdb test_ram.elf` `(gdb) target remote ip:port` `(gdb) load` | Load should return without error, typical output looks like: `Loading section .text, size 0x14c lma 0x0 Start address 0x40, load size 332 Transfer rate: 180 bytes/sec, 332 bytes/write.` | PASS/FAIL
DBG002 | Fill in! | Fill in! | Software breakpoint | Load the test_ram.elf application, use instructions from GDB001 | In the GDB console: `(gdb) monitor arm7_9 sw_bkpts enable software breakpoints enabled (gdb) break main Breakpoint 1 at 0xec: file src/main.c, line 71. (gdb) continue Continuing.` | The software breakpoint should be reached, a typical output looks like: `target state: halted target halted in ARM state due to breakpoint, current mode: Supervisor cpsr: 0x000000d3 pc: 0x000000ec Breakpoint 1, main () at src/main.c:71 71 DWORD a = 1;` | PASS/FAIL
DBG003 | Fill in! | Fill in! | Single step in a RAM application | Load the test_ram.elf application, use instructions from GDB001, break in main using the instructions from GDB002 | In GDB, type `(gdb) step` | The next instruction should be reached, typical output: `(gdb) step target state: halted target halted in ARM state due to single step, current mode: Abort cpsr: 0x20000097 pc: 0x000000f0 target state: halted target halted in ARM state due to single step, current mode: Abort cpsr: 0x20000097 pc: 0x000000f4 72 DWORD b = 2;` | PASS/FAIL
DBG004 | Fill in! | Fill in! | Software break points are working after a reset | Load the test_ram.elf application, use instructions from GDB001, break in main using the instructions from GDB002 | In GDB, type `(gdb) monitor reset (gdb) load (gdb) continue` | The breakpoint should be reached, typical output: `target state: halted target halted in ARM state due to breakpoint, current mode: Supervisor cpsr: 0x000000d3 pc: 0x000000ec Breakpoint 1, main () at src/main.c:71 71 DWORD a = 1;` | PASS/FAIL
DBG005 | Fill in! | Fill in! | Hardware breakpoint | Flash the test_rom.elf application. Make this test after FLA004 has passed | Be sure that `gdb_memory_map` and `gdb_flash_program` are enabled. In GDB, type `(gdb) monitor reset (gdb) load Loading section .text, size 0x194 lma 0x100000 Start address 0x100040, load size 404 Transfer rate: 179 bytes/sec, 404 bytes/write. (gdb) monitor arm7_9 force_hw_bkpts enable force hardware breakpoints enabled (gdb) break main Breakpoint 1 at 0x100134: file src/main.c, line 69. (gdb) continue` | The breakpoint should be reached, typical output: `Continuing. Breakpoint 1, main () at src/main.c:69 69 DWORD a = 1;` | PASS/FAIL
DBG006 | Fill in! | Fill in! | Hardware breakpoint is set after a reset | Follow the instructions to flash and insert a hardware breakpoint from DBG005 | In GDB, type `(gdb) monitor reset (gdb) monitor reg pc 0x100000 pc (/32): 0x00100000 (gdb) continue` | The breakpoint should be reached, typical output: `Continuing. Breakpoint 1, main () at src/main.c:69 69 DWORD a = 1;` | PASS/FAIL
DBG007 | Fill in! | Fill in! | Single step in ROM | Flash the test_rom.elf application and set a breakpoint in main, use DBG005. Make this test after FLA004 has passed | Be sure that `gdb_memory_map` and `gdb_flash_program` are enabled. In GDB, type `(gdb) monitor reset (gdb) load Loading section .text, size 0x194 lma 0x100000 Start address 0x100040, load size 404 Transfer rate: 179 bytes/sec, 404 bytes/write. (gdb) monitor arm7_9 force_hw_bkpts enable force hardware breakpoints enabled (gdb) break main Breakpoint 1 at 0x100134: file src/main.c, line 69. (gdb) continue Continuing. Breakpoint 1, main () at src/main.c:69 69 DWORD a = 1; (gdb) step` | The breakpoint should be reached, typical output: `target state: halted target halted in ARM state due to single step, current mode: Supervisor cpsr: 0x60000013 pc: 0x0010013c 70 DWORD b = 2;` | PASS/FAIL

## RAM access

Note: these tests are not designed to test/debug the target, but to test functionalities!

ID | Target | Interface | Description | Initial state | Input | Expected output | Pass/Fail
RAM001 | Fill in! | Fill in! | 32 bit Write/read RAM | Reset init is working | On the telnet interface `> mww ram_address 0xdeadbeef 16 > mdw ram_address 32` | The commands should execute without error. A clear failure is a memory access exception. The result of running the commands should be a list of 16 locations 32bit long containing 0xdeadbeef. `> mww 0x0 0xdeadbeef 16 > mdw 0x0 32 0x00000000: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x00000020: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x00000040: e1a00000 e59fa51c e59f051c e04aa000 00080017 00009388 00009388 00009388 0x00000060: 00009388 0002c2c0 0002c2c0 000094f8 000094f4 00009388 00009388 00009388` | PASS/FAIL
RAM001 | Fill in! | Fill in! | 16 bit Write/read RAM | Reset init is working | On the telnet interface `> mwh ram_address 0xbeef 16 > mdh ram_address 32` | The commands should execute without error. A clear failure is a memory access exception. The result of running the commands should be a list of 16 locations 16bit long containing 0xbeef. `> mwh 0x0 0xbeef 16 > mdh 0x0 32 0x00000000: beef beef beef beef beef beef beef beef beef beef beef beef beef beef beef beef 0x00000020: 00e0 0000 021c 0000 0240 0000 026c 0000 0288 0000 0000 0000 0388 0000 0350 0000 >` | PASS/FAIL
RAM003 | Fill in! | Fill in! | 8 bit Write/read RAM | Reset init is working | On the telnet interface `> mwb ram_address 0xab 16 > mdb ram_address 32` | The commands should execute without error. A clear failure is a memory access exception. The result of running the commands should be a list of 16 locations 8bit long containing 0xab. `> mwh 0x0 0x0 16 > mwb ram_address 0xab 16 > mdb ram_address 32 0x00000000: ab ab ab ab ab ab ab ab ab ab ab ab ab ab ab ab 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 >` | PASS/FAIL

## Flash access

ID | Target | Interface | Description | Initial state | Input | Expected output | Pass/Fail
FLA002 | Fill in! | Fill in! | flash fillw | Reset init is working, flash is probed | On the telnet interface `> flash fillw 0x1000000 0xdeadbeef 16` | The commands should execute without error. The output looks like: `wrote 64 bytes to 0x01000000 in 11.610000s (0.091516 kb/s)` To verify the contents of the flash: `> mdw 0x1000000 32 0x01000000: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x01000020: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x01000040: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x01000060: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff` | PASS/FAIL
FLA003 | Fill in! | Fill in! | Flash erase | Reset init is working, flash is probed | On the telnet interface `> flash erase_address 0x1000000 0x2000` | The commands should execute without error. `erased address 0x01000000 length 8192 in 4.970000s` To check that the flash has been erased, read at different addresses. The result should always be 0xff. `> mdw 0x1000000 32 0x01000000: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x01000020: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x01000040: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x01000060: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff` | PASS/FAIL
FLA004 | Fill in! | Fill in! | Loading to flash from GDB | Reset init is working, flash is probed, connectivity to GDB server is working | Start GDB using a ROM elf image, eg: arm-elf-gdb test_rom.elf. `(gdb) target remote ip:port (gdb) monitor reset (gdb) load Loading section .text, size 0x194 lma 0x100000 Start address 0x100040, load size 404 Transfer rate: 179 bytes/sec, 404 bytes/write. (gdb) monitor verify_image path_to_elf_file` | The output should look like: `verified 404 bytes in 5.060000s` The failure message is something like: `Verify operation failed address 0x00200000. Was 0x00 instead of 0x18` | PASS/FAIL