# SAM7

## Connectivity

ID | Target | Interface | Description | Initial state | Input | Expected output | Actual output | Pass/Fail
CON001 | AT91FR40162 | ZY1000 | Telnet connection | Power on, jtag target attached | On console, type `telnet ip port` | `Open On-Chip Debugger >` | `Open On-Chip Debugger >` | PASS
CON002 | AT91FR40162 | ZY1000 | GDB server connection | Power on, jtag target attached | On GDB console, type `target remote ip:port` | `Remote debugging using 10.0.0.73:3333` | `(gdb) tar remo 10.0.0.138:3333 Remote debugging using 10.0.0.138:3333 0x000155b8 in ?? ()` | PASS

## Reset

ID | Target | Interface | Description | Initial state | Input | Expected output | Actual output | Pass/Fail
RES001 | AT91FR40162 | ZY1000 | Reset halt on a blank target | Erase all the content of the flash | Connect via the telnet interface and type `reset halt` | Reset should return without error and the output should contain `target state: halted` | `> mdw 0x01000000 32 0x01000000: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x01000020: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x01000040: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x01000060: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff > reset halt JTAG tap: zy1000.cpu tap/device found: 0x1f0f0f0f (mfg: 0x787, part: 0xf0f0, ver: 0x1) srst pulls trst - can not reset into halted mode. Issuing halt after reset. target state: halted target halted in ARM state due to debug-request, current mode: Supervisor cpsr: 0x600000d3 pc: 0x00008a70 >` | PASS
RES002 | AT91FR40162 | ZY1000 | Reset init on a blank target | Erase all the content of the flash | Connect via the telnet interface and type `reset init` | Reset should return without error and the output should contain `executing reset script 'name_of_the_script'` | `> reset init JTAG tap: zy1000.cpu tap/device found: 0x1f0f0f0f (mfg: 0x787, part: 0xf0f0, ver: 0x1) srst pulls trst - can not reset into halted mode. Issuing halt after reset. target state: halted target halted in ARM state due to debug-request, current mode: Supervisor cpsr: 0x600000d3 pc: 0x00008ea4 >` | PASS NOTE! Even if there is no message, the reset script is being executed (proved by side effects)
RES003 | AT91FR40162 | ZY1000 | Reset after a power cycle of the target | Reset the target then power cycle the target | Connect via the telnet interface and type `reset halt` after the power was detected | Reset should return without error and the output should contain `target state: halted` | `Sensed nSRST asserted Sensed power dropout. target state: halted target halted in ARM state due to debug request, current mode: Supervisor cpsr: 0xf00000d3 pc: 0xd5dff7e6 Sensed power restore. Sensed nSRST deasserted > reset halt JTAG device found: 0x3f0f0f0f (Manufacturer: 0x787, Part: 0xf0f0, Version: 0x3) srst pulls trst - can not reset into halted mode. Issuing halt after reset. target state: halted target halted in ARM state due to debug request, current mode: Supervisor cpsr: 0xf00000d3 pc: 0x0000072c >` | PASS
RES004 | AT91FR40162 | ZY1000 | Reset halt on a blank target where reset halt is supported | Erase all the content of the flash | Connect via the telnet interface and type `reset halt` | Reset should return without error and the output should contain `target state: halted pc = 0` | > reset halt JTAG tap: zy1000.cpu tap/device found: 0x1f0f0f0f (mfg: 0x787, part: 0xf0f0, ver: 0x1) srst pulls trst - can not reset into halted mode. Issuing halt after reset. target state: halted target halted in ARM state due to debug-request, current mode: Supervisor cpsr: 0xf00000d3 pc: 0x00008b38 > | PASS
RES005 | AT91FR40162 | ZY1000 | Reset halt on a blank target using return clock | Erase all the content of the flash, set the configuration script to use RCLK | Connect via the telnet interface and type `reset halt` | Reset should return without error and the output should contain `target state: halted` | `N/A, At91EB40A does NOT have support for RCLK` | N/A

## JTAG Speed

ID | Target | ZY1000 | Description | Initial state | Input | Expected output | Actual output | Pass/Fail
SPD001 | AT91FR40162 | ZY1000 | 16MHz on normal operation | Reset init the target according to RES002 | Change speed and exercise a memory access over the JTAG, for example `mdw 0x0 32` | The command should run without any errors. If any JTAG checking errors happen, the test failed | `> reset halt JTAG tap: zy1000.cpu tap/device found: 0x1f0f0f0f (mfg: 0x787, part: 0xf0f0, ver: 0x1) srst pulls trst - can not reset into halted mode. Issuing halt after reset. target state: halted target halted in ARM state due to debug-request, current mode: Supervisor cpsr: 0xf00000d3 pc: 0x00008ae8 > jtag_khz 16000 jtag_speed 4 => JTAG clk=16.000000 16000 kHz > mdw 0 32 0x00000000: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000020: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000040: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000060: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff` | PASS
SPD002 | AT91FR40162 | ZY1000 | 8MHz on normal operation | Reset init the target according to RES002 | Change speed and exercise a memory access over the JTAG, for example `mdw 0x0 32` | The command should run without any errors. If any JTAG checking errors happen, the test failed | `> reset halt JTAG tap: zy1000.cpu tap/device found: 0x1f0f0f0f (mfg: 0x787, part: 0xf0f0, ver: 0x1) srst pulls trst - can not reset into halted mode. Issuing halt after reset. target state: halted target halted in ARM state due to debug-request, current mode: Supervisor cpsr: 0xf00000d3 pc: 0x00008c14 > jtag_khz 8000 jtag_speed 8 => JTAG clk=8.000000 8000 kHz > mdw 0 32 0x00000000: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000020: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000040: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000060: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff >` | PASS
SPD003 | AT91FR40162 | ZY1000 | 4MHz on normal operation | Reset init the target according to RES002 | Change speed and exercise a memory access over the JTAG, for example `mdw 0x0 32` | The command should run without any errors. If any JTAG checking errors happen, the test failed | `> reset halt JTAG tap: zy1000.cpu tap/device found: 0x1f0f0f0f (mfg: 0x787, part: 0xf0f0, ver: 0x1) srst pulls trst - can not reset into halted mode. Issuing halt after reset. target state: halted target halted in ARM state due to debug-request, current mode: Supervisor cpsr: 0xf00000d3 pc: 0x00008bc4 > jtag_khz 4000 jtag_speed 16 => JTAG clk=4.000000 4000 kHz > mdw 0 32 0x00000000: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000020: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000040: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000060: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff >` | PASS
SPD004 | AT91FR40162 | ZY1000 | 2MHz on normal operation | Reset init the target according to RES002 | Change speed and exercise a memory access over the JTAG, for example `mdw 0x0 32` | The command should run without any errors. If any JTAG checking errors happen, the test failed | `> reset halt JTAG tap: zy1000.cpu tap/device found: 0x1f0f0f0f (mfg: 0x787, part: 0xf0f0, ver: 0x1) srst pulls trst - can not reset into halted mode. Issuing halt after reset. target state: halted target halted in ARM state due to debug-request, current mode: Supervisor cpsr: 0xf00000d3 pc: 0x00009678 > jtag_khz 2000 jtag_speed 32 => JTAG clk=2.000000 2000 kHz > mdw 0 32 0x00000000: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000020: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000040: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x00000060: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff >` | PASS
SPD005 | AT91FR40162 | ZY1000 | RCLK on normal operation | Reset init the target according to RES002 | Change speed and exercise a memory access over the JTAG, for example `mdw 0x0 32` | The command should run without any errors. If any JTAG checking errors happen, the test failed | `> jtag_khz 0 RCLK - adaptive RCLK timeout` N/A for this target | N/A for this target

## Debugging

ID | Target | Interface | Description | Initial state | Input | Expected output | Actual output | Pass/Fail
DBG001 | AT91FR40162 | ZY1000 | Load is working | Reset init is working, RAM is accesible, GDB server is started | On the console of the OS: `$ arm-none-eabi-gdb redboot_ram.elf` `(gdb) target remote ip:port` `(gdb) load` | Load should return without error, typical output looks like: `Loading section .text, size 0x14c lma 0x0 Start address 0x40, load size 332 Transfer rate: 180 bytes/sec, 332 bytes/write.` | `(gdb) load Loading section .rom_vectors, size 0x40 lma 0xc000 Loading section .text, size 0x103e8 lma 0xc040 Loading section .rodata, size 0x1a84 lma 0x1c428 Loading section .data, size 0x3ec lma 0x1deac Start address 0xc040, load size 74392 Transfer rate: 572 KB/sec, 9299 bytes/write. (gdb)` | PASS
DBG002 | AT91FR40162 | ZY1000 | Software breakpoint | Load the redboot_ram.elf application, use instructions from GDB001 | In the GDB console: `(gdb) monitor arm7_9 dbgrq enable software breakpoints enabled (gdb) break cyg_start Breakpoint 1 at 0xec: file src/main.c, line 71. (gdb) continue Continuing.` | The software breakpoint should be reached, a typical output looks like: `Breakpoint 1, main () at src/main.c:69 69 DWORD a = 1;` | `(gdb) monitor arm7_9 dbgrq enable use of EmbeddedICE dbgrq instead of breakpoint for target halt enabled (gdb) break cyg_start Breakpoint 1 at 0x155b8: file /home/edgar/temp/ecosboard/packages/redboot/current/src/main.c, line 264. (gdb) continue Continuing. Breakpoint 1, cyg_start () at /home/edgar/temp/ecosboard/packages/redboot/current/src/main.c:264 264 CYGACC_CALL_IF_MONITOR_VERSION_SET(RedBoot_version); (gdb)` | PASS
DBG003 | AT91FR40162 | ZY1000 | Single step in a RAM application | Load the test_ram.elf application, use instructions from GDB001, break in main using the instructions from GDB002 | In GDB, type `(gdb) step` | The next instruction should be reached, typical output: `(gdb) step 70 DWORD b = 2;` | `(gdb) step 266 CYGACC_CALL_IF_MONITOR_RETURN_SET(return_to_redboot); (gdb)` | PASS
DBG004 | AT91FR40162 | ZY1000 | Software break points are working after a reset | Load the test_ram.elf application, use instructions from GDB001, break in main using the instructions from GDB002 | In GDB, type `(gdb) monitor reset init (gdb) load (gdb) continue` | The breakpoint should be reached, typical output: `Breakpoint 1, main () at src/main.c:69 69 DWORD a = 1;` | `(gdb) moni reset init JTAG tap: zy1000.cpu tap/device found: 0x1f0f0f0f (mfg: 0x787, part: 0xf0f0, ver: 0x1) srst pulls trst - can not reset into halted mode. Issuing halt after reset. target state: halted target halted in ARM state due to debug-request, current mode: Supervisor cpsr: 0x600000d3 pc: 0x00008ae8 (gdb) load Loading section .rom_vectors, size 0x40 lma 0xc000 Loading section .text, size 0x103e8 lma 0xc040 Loading section .rodata, size 0x1a84 lma 0x1c428 Loading section .data, size 0x3ec lma 0x1deac Start address 0xc040, load size 74392 Transfer rate: 576 KB/sec, 9299 bytes/write. (gdb) c Continuing. Breakpoint 1, cyg_start () at /home/edgar/temp/ecosboard/packages/redboot/current/src/main.c:264 264 CYGACC_CALL_IF_MONITOR_VERSION_SET(RedBoot_version); (gdb)` | PASS
DBG005 | AT91FR40162 | ZY1000 | Hardware breakpoint | Flash the redboot_rom.elf application. Make this test after FLA004 has passed | Be sure that `gdb_memory_map` and `gdb_flash_program` are enabled. In GDB, type `(gdb) monitor reset init (gdb) load Loading section .text, size 0x194 lma 0x100000 Start address 0x100040, load size 404 Transfer rate: 179 bytes/sec, 404 bytes/write. (gdb) monitor arm7_9 force_hw_bkpts enable force hardware breakpoints enabled (gdb) break main Breakpoint 1 at 0x100134: file src/main.c, line 69. (gdb) continue` | The breakpoint should be reached, typical output: `Continuing. Breakpoint 1, main () at src/main.c:69 69 DWORD a = 1;` | `(gdb) load Loading section .rom_vectors, size 0x40 lma 0x1000000 Loading section .text, size 0x10638 lma 0x1000040 Loading section .rodata, size 0x1a84 lma 0x1010678 Loading section .data, size 0x428 lma 0x10120fc Start address 0x1000040, load size 75044 Transfer rate: 33 KB/sec, 9380 bytes/write. (gdb) break cyg_start Breakpoint 1 at 0x100979c: file /home/edgar/temp/ecosboard/packages/redboot/current/src/main.c, line 264. (gdb) c Continuing. Note: automatically using hardware breakpoints for read-only addresses. Breakpoint 1, cyg_start () at /home/edgar/temp/ecosboard/packages/redboot/current/src/main.c:264 264 CYGACC_CALL_IF_MONITOR_VERSION_SET(RedBoot_version); (gdb)` | PASS
DBG006 | AT91FR40162 | ZY1000 | Hardware breakpoint is set after a reset | Follow the instructions to flash and insert a hardware breakpoint from DBG005 | In GDB, type `(gdb) monitor reset (gdb) monitor reg pc 0x100000 pc (/32): 0x00100000 (gdb) continue` where the value inserted in PC is the start address of the application | The breakpoint should be reached, typical output: `Continuing. Breakpoint 1, main () at src/main.c:69 69 DWORD a = 1;` | `(gdb) moni reset init JTAG tap: zy1000.cpu tap/device found: 0x1f0f0f0f (mfg: 0x787, part: 0xf0f0, ver: 0x1) srst pulls trst - can not reset into halted mode. Issuing halt after reset. target state: halted target halted in ARM state due to debug-request, current mode: Supervisor cpsr: 0x200000d3 pc: 0x01000200 (gdb) moni reg pc 0x1000000 pc (/32): 0x01000000 (gdb) c Continuing. Breakpoint 1, cyg_start () at /home/edgar/temp/ecosboard/packages/redboot/current/src/main.c:264 264 CYGACC_CALL_IF_MONITOR_VERSION_SET(RedBoot_version); (gdb)` | PASS
DBG007 | AT91FR40162 | ZY1000 | Single step in ROM | Flash the test_rom.elf application and set a breakpoint in main, use DBG005. Make this test after FLA004 has passed | Be sure that `gdb_memory_map` and `gdb_flash_program` are enabled. In GDB, type `(gdb) monitor reset (gdb) load Loading section .text, size 0x194 lma 0x100000 Start address 0x100040, load size 404 Transfer rate: 179 bytes/sec, 404 bytes/write. (gdb) monitor arm7_9 force_hw_bkpts enable force hardware breakpoints enabled (gdb) break main Breakpoint 1 at 0x100134: file src/main.c, line 69. (gdb) continue Continuing. Breakpoint 1, main () at src/main.c:69 69 DWORD a = 1; (gdb) step` | The breakpoint should be reached, typical output: `target state: halted target halted in ARM state due to single step, current mode: Supervisor cpsr: 0x60000013 pc: 0x0010013c 70 DWORD b = 2;` | `Breakpoint 1, cyg_start () at /home/edgar/temp/ecosboard/packages/redboot/current/src/main.c:264 264 CYGACC_CALL_IF_MONITOR_VERSION_SET(RedBoot_version); (gdb) step 266 CYGACC_CALL_IF_MONITOR_RETURN_SET(return_to_redboot);` | PASS

## RAM access

Note: these tests are not designed to test/debug the target, but to test functionalities!

ID | Target | Interface | Description | Initial state | Input | Expected output | Actual output | Pass/Fail
RAM001 | AT91FR40162 | ZY1000 | 32 bit Write/read RAM | Reset init is working | On the telnet interface `> mww ram_address 0xdeadbeef 16 > mdw ram_address 32` | The commands should execute without error. A clear failure is a memory access exception. The result of running the commands should be a list of 16 locations 32bit long containing 0xdeadbeef. `> mww 0x0 0xdeadbeef 16 > mdw 0x0 32 0x00000000: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x00000020: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x00000040: e1a00000 e59fa51c e59f051c e04aa000 00080017 00009388 00009388 00009388 0x00000060: 00009388 0002c2c0 0002c2c0 000094f8 000094f4 00009388 00009388 00009388` | `> mww 0 0xdeadbeef 16 > mdw 0x0 32 0x00000000: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x00000020: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x00000040: 15aadc6d 425b6f33 e789f955 d390dcc2 00080017 010067b4 010067b4 010067b4 0x00000060: 010067b4 00006e74 00006e74 010067b4 010067b4 010067b4 010067b4 010067b4` | PASS
RAM002 | AT91FR40162 | ZY1000 | 16 bit Write/read RAM | Reset init is working | On the telnet interface `> mwh ram_address 0xbeef 16 > mdh ram_address 32` | The commands should execute without error. A clear failure is a memory access exception. The result of running the commands should be a list of 16 locations 16bit long containing 0xbeef. `> mwh 0x0 0xbeef 16 > mdh 0x0 32 0x00000000: beef beef beef beef beef beef beef beef beef beef beef beef beef beef beef beef 0x00000020: 00e0 0000 021c 0000 0240 0000 026c 0000 0288 0000 0000 0000 0388 0000 0350 0000 >` | `> mwh 0 0xbeef 16 > mdh 0x0 32 0x00000000: beef beef beef beef beef beef beef beef beef beef beef beef beef beef beef beef 0x00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00` | PASS There is a problem with the formatting of the output
RAM003 | AT91FR40162 | ZY1000 | 8 bit Write/read RAM | Reset init is working | On the telnet interface `> mwb ram_address 0xab 16 > mdb ram_address 32` | The commands should execute without error. A clear failure is a memory access exception. The result of running the commands should be a list of 16 locations 8bit long containing 0xab. `> mwb ram_address 0xab 16 > mdb ram_address 32 0x00000000: ab ab ab ab ab ab ab ab ab ab ab ab ab ab ab ab 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 >` | `> mwb 0x0 0xab 16 > mdb 0x0 32 0x00000000: ab ab ab ab ab ab ab ab ab ab ab ab ab ab ab ab 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00` | PASS

## Flash access

ID | Target | Interface | Description | Initial state | Input | Expected output | Actual output | Pass/Fail
FLA001 | AT91FR40162 | ZY1000 | Flash probe | Reset init is working | On the telnet interface: `> flash probe 0` | The command should execute without error. The output should state the name of the flash and the starting address. An example of output: `flash 'ecosflash' found at 0x01000000` | `> flash probe 0 flash 'ecosflash' found at 0x01000000` | PASS
FLA002 | AT91FR40162 | ZY1000 | flash fillw | Reset init is working, flash is probed | On the telnet interface `> flash fillw 0x100000 0xdeadbeef 16` | The commands should execute without error. The output looks like: `wrote 64 bytes to 0x0100000 in 11.610000s (0.091516 kb/s)` To verify the contents of the flash: `> mdw 0x100000 32 0x0100000: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x0100020: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x0100040: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x0100060: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff` | `> flash fillw 0x01000000 0xdeadbeef 16 wrote 64 bytes to 0x01000000 in 0.010000s (6.250 kb/s) > mdw 0x1000000 32 0x01000000: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x01000020: deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef deadbeef 0x01000040: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x01000060: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff >` | PASS
FLA003 | AT91FR40162 | ZY1000 | Flash erase | Reset init is working, flash is probed | On the telnet interface `> flash erase_address 0x100000 0x2000` | The commands should execute without error. `erased address 0x0100000 length 8192 in 4.970000s` To check that the flash has been erased, read at different addresses. The result should always be 0xff. `> mdw 0x100000 32 0x0100000: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x0100020: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x0100040: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x0100060: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff` | `> flash erase_address 0x1000000 0x10000 erased address 0x01000000 (length 65536) in 0.840000s (76.190 kb/s) > mdw 0x1000000 32 0x01000000: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x01000020: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x01000040: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff 0x01000060: ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff ffffffff` | PASS
FLA004 | AT91FR40162 | ZY1000 | Loading to flash from GDB | Reset init is working, flash is probed, connectivity to GDB server is working | Start GDB using a ROM elf image, eg: arm-elf-gdb test_rom.elf. `(gdb) target remote ip:port (gdb) monitor reset halt (gdb) load Loading section .text, size 0x194 lma 0x100000 Start address 0x100040, load size 404 Transfer rate: 179 bytes/sec, 404 bytes/write. (gdb) monitor verify_image path_to_elf_file` | The output should look like: `verified 404 bytes in 5.060000s` The failure message is something like: `Verify operation failed address 0x00200000. Was 0x00 instead of 0x18` | `(gdb) load Loading section .rom_vectors, size 0x40 lma 0x1000000 Loading section .text, size 0x10638 lma 0x1000040 Loading section .rodata, size 0x1a84 lma 0x1010678 Loading section .data, size 0x428 lma 0x10120fc Start address 0x1000040, load size 75044 Transfer rate: 34 KB/sec, 9380 bytes/write. (gdb) moni verify_image /tftp/10.0.0.190/redboot_rom.elf keep_alive() was not invoked in the 1000ms timelimit. GDB alive packet not sent! (1820). Workaround: increase "set remotetimeout" in GDB verified 75044 bytes in 1.960000s (37.390 kb/s)` | PASS